# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="OnePlus 5"
deviceinfo_manufacturer="OnePlus"
deviceinfo_codename="oneplus-cheeseburger"
deviceinfo_year="2017"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_drm="true"
deviceinfo_chassis="handset"
deviceinfo_external_storage="false"
deviceinfo_screen_width="1080"
deviceinfo_screen_height="1920"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt="false"
deviceinfo_flash_offset_base="0x00000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x01000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_pagesize="4096"
deviceinfo_flash_sparse="true"

# Required for devices using UFS as storage (instead of e.g. eMMC)
deviceinfo_rootfs_image_sector_size="4096"

# Common mainline kernel options
deviceinfo_flash_kernel_on_update="true"
deviceinfo_dtb="qcom/msm8998-oneplus-cheeseburger"
deviceinfo_append_dtb="true"

# Close to mainline kernel options
# We need 'clk_ignore_unused' for now or we don't get graphics

# Alpine kernel options

