# Based on arch/arm64/boot/dts/qcom/spi-panel-gc9307-hlt-28-qvga-cmd.dtsi from
# the downstream kernel, which is:
# Copyright (c) 2017, 2020, The Linux Foundation. All rights reserved.
#
# This program is free software; you can redistribute it and/or modify
# it under the terms of the GNU General Public License version 2 and
# only version 2 as published by the Free Software Foundation.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.

command 0x11 # exit sleep mode
delay 120
command 0xfe
command 0xef
command 0x13
command 0x38
command 0x20
command 0x36 0x00
command 0x3a 0x05
command 0x35 0x00
command 0x89 0x0b
command 0xeb 0x02
command 0x29 # display on
