# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="BananaPi BPI-CM4IO Baseboard with BPI-CM4"
deviceinfo_manufacturer="BananaPi"
deviceinfo_codename="bananapi-bpi-cm4-cm4io"
deviceinfo_dtb="amlogic/meson-g12b-bananapi-cm4-cm4io"
deviceinfo_year="2023"
deviceinfo_arch="aarch64"
deviceinfo_disable_dhcpd="true"
deviceinfo_partition_type="msdos"

# Device related
deviceinfo_drm="true"
deviceinfo_chassis="desktop"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1920"
deviceinfo_screen_height="1080"

# Bootloader related
deviceinfo_sd_embed_firmware_step_size="512"
deviceinfo_sd_embed_firmware="u-boot/bananapi-bpi-cm4-cm4io/u-boot.bin.sd-stripped.bin:1"
deviceinfo_boot_part_start="4096"
deviceinfo_generate_extlinux_config="true"
# Kernel options

