From 1e5fd2de0d75e585c3e8bdaffc9a8dfcf647c51b Mon Sep 17 00:00:00 2001
From: Ferass El Hafidi <funderscore@postmarketos.org>
Date: Sun, 2 Feb 2025 14:14:03 +0000
Subject: [PATCH 1/2] dt-bindings: arm: amlogic: add S805Y and Mi TV Stick

Add support for the Amlogic S805Y SoC and the Xiaomi Mi TV Stick (aka.
xiaomi-aquaman).  The S805Y is very similar to the S805X, with just a
few minor differences.

Acked-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Reviewed-by: Martin Blumenstingl <martin.blumenstingl@googlemail.com>
Signed-off-by: Ferass El Hafidi <funderscore@postmarketos.org>
---
 Documentation/devicetree/bindings/arm/amlogic.yaml | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/Documentation/devicetree/bindings/arm/amlogic.yaml b/Documentation/devicetree/bindings/arm/amlogic.yaml
index 0c84c5685..befc51765 100644
--- a/Documentation/devicetree/bindings/arm/amlogic.yaml
+++ b/Documentation/devicetree/bindings/arm/amlogic.yaml
@@ -73,6 +73,13 @@ properties:
           - const: amlogic,s805x
           - const: amlogic,meson-gxl
 
+      - description: Boards with the Amlogic Meson GXL S805Y SoC
+        items:
+          - enum:
+              - xiaomi,aquaman
+          - const: amlogic,s805y
+          - const: amlogic,meson-gxl
+
       - description: Boards with the Amlogic Meson GXL S905W SoC
         items:
           - enum:
-- 
2.49.0

