# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Samsung Galaxy A51"
deviceinfo_manufacturer="Samsung"
deviceinfo_codename="samsung-a51"
deviceinfo_year="2019"
deviceinfo_dtb="exynos9610"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_chassis="handset"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1080"
deviceinfo_screen_height="2400"

# Bootloader related
deviceinfo_flash_method="heimdall-bootimg"
deviceinfo_generate_bootimg="true"
deviceinfo_flash_pagesize="2048"
deviceinfo_header_version="2"
deviceinfo_append_dtb="false"
deviceinfo_bootimg_qcdt="false"
deviceinfo_flash_offset_dtb="0x00000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x01000000"
deviceinfo_flash_offset_second="0xf0000000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_heimdall_partition_kernel="boot"
deviceinfo_flash_heimdall_partition_rootfs="super"

# Dynamic partition (super)
deviceinfo_super_partitions="/dev/sda25 /dev/sda25"

# USB
deviceinfo_usb_idProduct="0x685d"
deviceinfo_usb_idVendor="0x04e8"
