# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Clockwork Tech ClockworkPi uConsole Radxa CM5"
deviceinfo_manufacturer="Clockwork Tech"
deviceinfo_codename="clockworkpi-uconsole-radxa-cm5"
deviceinfo_year="2023"
deviceinfo_arch="aarch64"
deviceinfo_disable_dhcpd="true"

# Device related
deviceinfo_drm="true"
deviceinfo_chassis="embedded"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1280"
deviceinfo_screen_height="720"
deviceinfo_getty="ttyFIQ0;1500000"

# Bootloader related
deviceinfo_boot_filesystem="fat32"
deviceinfo_dtb="rockchip/rk3588s-radxa-cm5-uconsole"
deviceinfo_sd_embed_firmware="u-boot/radxa-cm5/rpi-cm4-io/idbloader.img:64,u-boot/radxa-cm5/rpi-cm4-io/u-boot.itb:16384"
deviceinfo_sd_embed_firmware_step_size="512"
deviceinfo_boot_part_start="32768"
deviceinfo_generate_extlinux_config="true"
