From c866f097c4684d183ceb9f5812924916377040d7 Mon Sep 17 00:00:00 2001
From: Daniele Debernardi <drebrez@gmail.com>
Date: Wed, 4 Nov 2020 01:50:15 +0100
Subject: [PATCH] Fix decon_reg variable type

---
 drivers/video/fbdev/exynos/dpu/decon_reg.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/video/fbdev/exynos/dpu/decon_reg.c b/drivers/video/fbdev/exynos/dpu/decon_reg.c
index 589d79f8fed8..226e601cc8a0 100644
--- a/drivers/video/fbdev/exynos/dpu/decon_reg.c
+++ b/drivers/video/fbdev/exynos/dpu/decon_reg.c
@@ -2588,7 +2588,7 @@ u32 decon_reg_get_height(u32 id, int dsi_mode)
 	return (FORMATTER_HEIGHT_GET(val));
 }
 
-const double decon_clocks_table[][CLK_ID_MAX] = {
+const unsigned long decon_clocks_table[][CLK_ID_MAX] = {
 	/* VCLK,  ECLK,  ACLK,  PCLK,  DISP_PLL,  resolution,            MIC_ratio, DSC count */
 	{    71,   168,   400,    66,        71, 1080 * 1920,     MIC_COMP_BYPASS,         0},
 	{    63,   168,   400,    66,        63, 1440 * 2560,  MIC_COMP_RATIO_1_2,         0},
-- 
2.50.0

