# Maintainer: He Yangxuan <yangxuan8282@gmail.com>

pkgname=bluetooth-raspberry-pi
pkgver=1
pkgrel=0
pkgdesc="Service and udev rule for built-in bluetooth on Raspberry Pi zero w, 3B, 3B plus"
url="https://github.com/RPi-Distro/bluez-firmware"
arch="armhf aarch64"
license="MIT"
depends="bluez bluez-deprecated"
install="$pkgname.post-install"
source="pi-bluetooth.openrc 50-bluetooth-hci-auto-poweron.rules"
options="!check !archcheck"

package() {
	cd "$srcdir"
	install -Dm644 50-bluetooth-hci-auto-poweron.rules "$pkgdir"/etc/udev/rules.d/50-bluetooth-hci-auto-poweron.rules
	install -Dm755 pi-bluetooth.openrc "$pkgdir"/etc/init.d/pi-bluetooth
}

sha512sums="34a50554466dd6096cbee9b14fc0d77b268b731cd45981e69394343dad25d6006dbe44bee30700d71b80c593d38699dfc870983ae7d862b9c09afb39c5d3b383  pi-bluetooth.openrc
511281ae8cbebd4390836ba83049a7fb793121d60ebd6c436bf36330e0aab738a827daf7fd6721cc71681e72b7ddaa581814264cc3bf759f07148fe5b657b981  50-bluetooth-hci-auto-poweron.rules"
