# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Motorola One Hyper"
deviceinfo_manufacturer="Motorola"
deviceinfo_codename="motorola-def"
deviceinfo_year="2019"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_no_framebuffer="true"
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1080"
deviceinfo_screen_height="2340"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_kernel_cmdline="console=ttyMSM0,115200n8 androidboot.hardware=qcom androidboot.console=ttyMSM0 androidboot.memcg=1 lpm_levels.sleep_disabled=1 video=vfb:640x400,bpp=32,memsize=3072000 msm_rtb.filter=0x237 service_locator.enable=1 swiotlb=1 androidboot.usbcontroller=a600000.dwc3 earlycon=msm_geni_serial,0x880000 loop.max_part=7 printk.devkmsg=on androidboot.hab.csv=0 androidboot.hab.product=def androidboot.hab.cid=50 firmware_class.path=/vendor/firmware_mnt/image buildvariant=user"
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt="false"
deviceinfo_bootimg_dtb_second="false"
deviceinfo_flash_offset_base="0x00000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x01000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_pagesize="4096"

