diff --git a/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts b/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
index e50bb54a4209..fceb5934d592 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
@@ -1338,7 +1338,7 @@ display_pwren1: display-pwren1 {
 
 	stk3311 {
 		stk3311_int: stk3311-int {
-			rockchip,pins = <4 RK_PD3 RK_FUNC_GPIO &pcfg_input_pull_up>;
+			rockchip,pins = <4 RK_PD3 RK_FUNC_GPIO &pcfg_input_enable>;
 		};
 	};
 
