# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Microsoft Surface RT"
deviceinfo_manufacturer="Microsoft"
deviceinfo_codename="microsoft-surface-rt"
deviceinfo_year="2012"
deviceinfo_dtb="tegra30-microsoft-surface-rt-efi"
deviceinfo_modules_initfs="surface-rt-ec hid-generic i2c-hotplug-gpio i2c-hid-of lvds-codec panel-lvds"
deviceinfo_arch="armv7"

# Device related
deviceinfo_chassis="tablet"
deviceinfo_keyboard="true"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1366"
deviceinfo_screen_height="768"
deviceinfo_dev_internal_storage="/dev/mmcblk0"
deviceinfo_dev_internal_storage_repartition="true"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_generate_bootimg="false"
deviceinfo_boot_filesystem="fat32"
