# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Beelink gt1 (Ultimate)"
deviceinfo_manufacturer="Beelink"
deviceinfo_codename="beelink-gt1"
deviceinfo_dtb="amlogic/meson-gxm-gt1-ultimate"
deviceinfo_year="2016"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_gpu_accelerated="true"
deviceinfo_chassis="desktop"
deviceinfo_keyboard="true"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1920"
deviceinfo_screen_height="1080"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_sd_embed_firmware_step_size="512"
deviceinfo_sd_embed_firmware="u-boot/beelink-gt1/u-boot.bin.sd-stripped.bin:1"
deviceinfo_boot_part_start="4096"
deviceinfo_generate_extlinux_config="true"
# Close to mainline kernel options
deviceinfo_modules_initfs_amlogic="meson_drm meson_dw_hdmi display_connector"
deviceinfo_kernel_cmdline_amlogic="rw console=ttyAML0,115200 console=tty0 PMOS_NO_OUTPUT_REDIRECT no_console_suspend"

# Alpine kernel options
deviceinfo_kernel_cmdline_alpine="rw console=ttyAML0,115200 console=tty0 PMOS_NO_OUTPUT_REDIRECT no_console_suspend"
deviceinfo_modules_initfs_alpine="fixed meson_gxbb_wdt meson_wdt meson-gx-mmc dw_hdmi drm_display_helper cec display_connector drm_kms_helper drm meson_drm meson_dw_hdmi"

