# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Purism Librem 5 Phone"
deviceinfo_manufacturer="Purism"
deviceinfo_codename="purism-librem5"
deviceinfo_year="2019"
deviceinfo_dtb="freescale/imx8mq-librem5-r2 freescale/imx8mq-librem5-r3 freescale/imx8mq-librem5-r4"
deviceinfo_append_dtb="false"
deviceinfo_modules_initfs="dwc3 edt-ft5x06 goodix gpio_vibra led_bl libcomposite phy_fsl_imx8mq_usb pwm_vibra tps6598x udc_core usbhid xhci_hcd xhci_plat_hcd bq25890_charger usb_storage uas snvs_pwrkey imx_sdma ofpart spi_nor"
deviceinfo_arch="aarch64"
deviceinfo_mesa_driver="mxsfb-drm"

# Device related
deviceinfo_gpu_accelerated="true"
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="720"
deviceinfo_screen_height="1440"

# Bootloader related
deviceinfo_flash_method="uuu"
deviceinfo_generate_legacy_uboot_initfs="false"
deviceinfo_sd_embed_firmware="u-boot/librem5/phone-boot.img:33"
deviceinfo_boot_part_start="4096"
