based on: https://patchwork.kernel.org/project/linux-mediatek/patch/20211213162856.235130-2-hsinyi@chromium.org/

diff --git a/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku0.dts b/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku0.dts
new file mode 100644
index 00000000000000..51bf2893ec03b1
--- /dev/null
+++ b/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku0.dts
@@ -0,0 +1,24 @@
+// SPDX-License-Identifier: (GPL-2.0 OR MIT)
+/*
+ * Copyright 2021 Google LLC
+ */
+
+/dts-v1/;
+#include "mt8183-kukui-jacuzzi-fennel.dtsi"
+#include "mt8183-kukui-audio-da7219-rt1015p.dtsi"
+
+/ {
+	model = "Google makomo sku0 board";
+	compatible = "google,makomo-rev4-sku0", "google,makomo-rev5-sku0",
+		"google,makomo", "mediatek,mt8183";
+};
+
+&qca_wifi {
+	qcom,ath10k-calibration-variant = "GO_FENNEL14";
+};
+
+&mmc1_pins_uhs {
+	pins_clk {
+		drive-strength = <MTK_DRIVE_6mA>;
+	};
+};
diff --git a/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku1.dts b/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku1.dts
new file mode 100644
index 00000000000000..c3b7e9bb0c8960
--- /dev/null
+++ b/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku1.dts
@@ -0,0 +1,24 @@
+// SPDX-License-Identifier: (GPL-2.0 OR MIT)
+/*
+ * Copyright 2021 Google LLC
+ */
+
+/dts-v1/;
+#include "mt8183-kukui-jacuzzi-fennel.dtsi"
+#include "mt8183-kukui-audio-ts3a227e-rt1015p.dtsi"
+
+/ {
+	model = "Google makomo sku1 board";
+	compatible = "google,makomo-rev4-sku1", "google,makomo-rev5-sku1",
+		"google,makomo", "mediatek,mt8183";
+};
+
+&qca_wifi {
+	qcom,ath10k-calibration-variant = "GO_FENNEL14";
+};
+
+&mmc1_pins_uhs {
+	pins_clk {
+		drive-strength = <MTK_DRIVE_6mA>;
+	};
+};
