# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="ASUS ZenWatch 2"
deviceinfo_manufacturer="ASUS"
deviceinfo_codename="asus-sparrow"
deviceinfo_year="2015"
deviceinfo_dtb_mainline="qcom-apq8026-asus-sparrow"
deviceinfo_append_dtb_mainline="true"
deviceinfo_arch="armv7"

# Device related
deviceinfo_chassis="watch"
deviceinfo_keyboard="false"
deviceinfo_external_storage="false"
deviceinfo_screen_width="320"
deviceinfo_screen_height="320"

# Bootloader related
deviceinfo_flash_method="fastboot"
# limit to single-core until we have cpufreq to avoid fast overheating
deviceinfo_kernel_cmdline_mainline="maxcpus=1"
deviceinfo_kernel_cmdline_downstream="console=ttyHSL0,115200,n8 androidboot.console=ttyHSL0 androidboot.hardware=sparrow user_debug=31 maxcpus=4 msm_rtb.filter=0x3F"
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt="false"
deviceinfo_bootimg_mtk_mkimage="false"
deviceinfo_bootimg_dtb_second="false"
deviceinfo_flash_pagesize="2048"
deviceinfo_flash_offset_base="0x00000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x02000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x01e00000"
