# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Sipeed Lichee Zero"
deviceinfo_manufacturer="Sipeed"
deviceinfo_codename="sipeed-licheezero"
deviceinfo_year="2017"
deviceinfo_modules_initfs="configfs roles musb_hdrc"
deviceinfo_arch="armv7"

# Device related
deviceinfo_chassis="embedded"
deviceinfo_keyboard="true"
deviceinfo_external_storage="true"
deviceinfo_screen_width="320"
deviceinfo_screen_height="240"
deviceinfo_getty="ttyS0;115200"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_sd_embed_firmware="u-boot/LicheePi_Zero/u-boot-sunxi-with-spl.bin:8"
