# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Xiaomi Mi A1"
deviceinfo_manufacturer="Xiaomi"
deviceinfo_codename="xiaomi-tissot"
deviceinfo_year="2017"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_gpu_accelerated="true"
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1080"
deviceinfo_screen_height="1920"
deviceinfo_swap_size_recommended="512"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_kernel_cmdline="earlycon console=null PMOS_NO_OUTPUT_REDIRECT"
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt="false"
deviceinfo_bootimg_dtb_second="false"
deviceinfo_flash_offset_base="0x80000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x01000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_pagesize="2048"
deviceinfo_flash_sparse="true"

# Kernel options
deviceinfo_dtb="qcom/msm8953-xiaomi-tissot"
deviceinfo_append_dtb="true"
deviceinfo_flash_kernel_on_update="false"

# osk-sdl
deviceinfo_modules_initfs="edt_ft5x06 msm panel-mdss-ili7807-fhd panel-mdss-otm1911-fhd panel-mdss-ft8716-fhd"
deviceinfo_mesa_driver="msm"
