# Maintainer: exkc <exxxxkc@getgoogleoff.me>
# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Xiaomi Mi Box 3"
deviceinfo_manufacturer="Xiaomi"
deviceinfo_codename="xiaomi-once"
deviceinfo_year="2016"
deviceinfo_dtb="amlogic/meson-gxl-s905x-xiaomi-once"
deviceinfo_modules_initfs="meson_drm meson_dw_hdmi display_connector"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_chassis="desktop"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="800"
deviceinfo_screen_height="600"
deviceinfo_gpu_accelerated="true"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_generate_extlinux_config="true"
deviceinfo_kernel_cmdline="rw console=ttyAML0,115200 PMOS_NO_OUTPUT_REDIRECT no_console_suspend"
