# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Kobo Libra H2O"
deviceinfo_manufacturer="Kobo"
deviceinfo_codename="kobo-librah2o"
deviceinfo_year="2019"
deviceinfo_arch="armv7"
deviceinfo_dtb="imx6sll-kobo-librah2o"
deviceinfo_drm="true"

# Device related
deviceinfo_chassis="tablet"
# eMMC can be exported as mass storage
deviceinfo_external_storage="true"
deviceinfo_screen_width="1264"
deviceinfo_screen_height="1680"

# Bootloader related
deviceinfo_boot_part_start="49152"
deviceinfo_getty="ttymxc0;115200"
deviceinfo_generate_legacy_uboot_initfs="true"
deviceinfo_no_framebuffer="true"

# GPT is supported, but bootloader location conflict with default GPT header
# location and specifying a custom location is not supported here yet
deviceinfo_partition_type="msdos"

deviceinfo_sd_embed_firmware_step_size="512"
deviceinfo_sd_embed_firmware="u-boot/kobo-librah2o/u-boot.imx:2,u-boot/kobo-librah2o/u-boot-env.bin:1536"
