# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Xunlong Orange Pi PC"
deviceinfo_manufacturer="Xunlong"
deviceinfo_codename="xunlong-orangepi-pc"
deviceinfo_year="2015"
deviceinfo_dtb="sun8i-h3-orangepi-pc"
deviceinfo_arch="armv7"
deviceinfo_disable_dhcpd="true"

# Device related
deviceinfo_drm="true"
deviceinfo_chassis="embedded"
deviceinfo_external_storage="true"
deviceinfo_screen_width="800"
deviceinfo_screen_height="600"
deviceinfo_getty="ttyS0;115200"

# Bootloader related
deviceinfo_generate_extlinux_config="true"
deviceinfo_sd_embed_firmware="u-boot/orangepi_pc/u-boot-sunxi-with-spl.bin:8"
