# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Pine64 Quartz64"
deviceinfo_manufacturer="Pine64"
deviceinfo_codename="pine64-quartz64"
deviceinfo_year="2021"
deviceinfo_dtb_a="rockchip/rk3566-quartz64-a"
deviceinfo_dtb_b="rockchip/rk3566-quartz64-b"
deviceinfo_arch="aarch64"
deviceinfo_drm="true"

# Device related
deviceinfo_chassis="embedded"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1920"
deviceinfo_screen_height="1080"
deviceinfo_getty="ttyS2;1500000"

# Bootloader related
deviceinfo_flash_method="rkdeveloptool"
deviceinfo_flash_sparse="true"

deviceinfo_boot_part_start="65536"

deviceinfo_sd_embed_firmware="u-boot/u-boot-rockchip-quartz64.bin:1"
deviceinfo_sd_embed_firmware_step_size="32768"

deviceinfo_generate_extlinux_config="true"
