From 31c9667cbc59c8711ed77cc4a260d0acc0dada3a Mon Sep 17 00:00:00 2001
From: Henrik Grimler <henrik@grimler.se>
Date: Mon, 23 Jun 2025 16:20:26 +0200
Subject: [PATCH] Fix display colors, use RGB instead of BGR

---
 drivers/video/fbdev/exynos/dpu/decon_dsi.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/drivers/video/fbdev/exynos/dpu/decon_dsi.c b/drivers/video/fbdev/exynos/dpu/decon_dsi.c
index eeaa2ba19778..b9ddbdf96716 100644
--- a/drivers/video/fbdev/exynos/dpu/decon_dsi.c
+++ b/drivers/video/fbdev/exynos/dpu/decon_dsi.c
@@ -862,11 +862,11 @@ int decon_check_var(struct fb_var_screeninfo *var, struct fb_info *info)
 	case 24:
 		/* our 24bpp is unpacked, so 32bpp */
 		var->bits_per_pixel	= 32;
-		var->red.offset		= 16;
+		var->red.offset		= 0;
 		var->red.length		= 8;
 		var->green.offset	= 8;
 		var->green.length	= 8;
-		var->blue.offset	= 0;
+		var->blue.offset	= 16;
 		var->blue.length	= 8;
 		break;
 
-- 
2.50.0

