# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Ouya"
deviceinfo_manufacturer="Ouya"
deviceinfo_codename="ouya-ouya-downstream"
deviceinfo_year="2013"
deviceinfo_chassis="embedded"
deviceinfo_flash_method="fastboot"
deviceinfo_arch="armv7"

# boot.img must be <=8MB to work with ouya_bootmenu
deviceinfo_create_initfs_extra="true"

# Splash screen
deviceinfo_screen_width="1920"
deviceinfo_screen_height="1080"

# Fastboot related
deviceinfo_generate_bootimg="true"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x01000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_pagesize="2048"
deviceinfo_partition_blacklist="boot,recovery"
