# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Google Pixel 4"
deviceinfo_manufacturer="Google"
deviceinfo_codename="google-flame"
deviceinfo_year="2019"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_chassis="handset"
deviceinfo_drm="true"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_getty="ttyMSM0;115200"
deviceinfo_boot_filesystem="fat32"
deviceinfo_dtb="qcom/sm8150-google-flame"

# Required for devices using UFS as storage (instead of e.g. eMMC)
deviceinfo_rootfs_image_sector_size="4096"

# Load super partitions
deviceinfo_super_partitions="/dev/sda14 /dev/sda14"

# Google Inc. Nexus/Pixel Device (tether)
deviceinfo_usb_idVendor="0x18d1"
deviceinfo_usb_idProduct="0x4ee3"
