# Archived: unmaintained
maintainer=""
pkgname=firmware-oneplus-oneplus3t
pkgver=2
pkgrel=1
pkgdesc="Firmware for OnePlus 3T"
url="https://gitlab.com/DrGit/firmware-oneplus3"
arch="aarch64"
license="proprietary"
makedepends="mtools pil-squasher qca-swiss-army-knife"
options="!check !strip !archcheck !tracedeps pmb:cross-native"
replaces="linux-firmware-ath10k"
_gpufw="https://github.com/TheMuppets/proprietary_vendor_oneplus/raw/lineage-17.1/oneplus3/proprietary/vendor/firmware"
_files="adsp.b00
	adsp.b01
	adsp.b02
	adsp.b03
	adsp.b04
	adsp.b05
	adsp.b06
	adsp.b08
	adsp.b09
	adsp.mdt
	bdwlan30.bin
	modem.b00
	modem.b01
	modem.b02
	modem.b03
	modem.b04
	modem.b05
	modem.b06
	modem.b07
	modem.b08
	modem.b09
	modem.b10
	modem.b11
	modem.b12
	modem.b13
	modem.b15
	modem.b16
	modem.b17
	modem.b18
	modem.b19
	modem.b20
	modem.mdt
	mba.mbn
	slpi.b00
	slpi.b01
	slpi.b02
	slpi.b03
	slpi.b04
	slpi.b05
	slpi.b06
	slpi.b07
	slpi.b08
	slpi.b09
	slpi.b10
	slpi.b11
	slpi.b12
	slpi.b13
	slpi.b14
	slpi.mdt
	venus.b00
	venus.b01
	venus.b02
	venus.b03
	venus.b04
	venus.mdt
"
source="$pkgname-$pkgver-NON-HLOS.bin::$url/-/raw/master/oneplus3t/NON-HLOS.bin
	$_gpufw/a530_zap-pro.elf
	20-adreno-gpu-firmware.files
	board-2.json
"

_mdtnames="adsp modem slpi venus"
_mbns="a530_zap.mbn adsp.mbn mba.mbn modem.mbn slpi.mbn venus.mbn"

unpack() {
	# Extract blobs
	for _i in $_files; do
		mcopy -v -b -p -n -i $srcdir/$pkgname-$pkgver-NON-HLOS.bin ::image/$_i $_i
	done
}

package() {
	# Squash firmware segments into mbns
	for _i in $_mdtnames; do
		pil-squasher "$_i.mbn" "$_i.mdt"
	done

	# Move zap shader to the same directory as the other mbns
	mv "$srcdir/a530_zap-pro.elf" "a530_zap.mbn"

	# Install mbns
	for _i in $_mbns; do
		install -Dm644 $_i "$pkgdir/lib/firmware/qcom/msm8996/oneplus3t/$_i"
	done

	# Install 20-adreno-gpu-firmware.files
	install -Dm644 "$srcdir/20-adreno-gpu-firmware.files" \
		"$pkgdir/usr/share/mkinitfs/files/20-adreno-gpu-firmware.files"

	# Create and install ath10k board file
	ath10k-bdencoder -c board-2.json
	install -Dm644 board-2.bin -t "$pkgdir/lib/firmware/ath10k/QCA6174/hw3.0"
}

sha512sums="
3da90f51fc39c3db4f0f39c07eda318b0b1fc85f7fbb8f21bd31a3ae5c73a4b39ba630a9521a7c5ee844e14c24d084f5d42e4c2ffd2bdee541e50ec7b1629b14  firmware-oneplus-oneplus3t-2-NON-HLOS.bin
237c82252f1ff44a454bed5f84a8dcf74e0f6ea6e5674e7d5aa32436fcf20d8c9df5c6edc4b4bc151e5fdce4694c1d14edc8ba0804ceb738f3fb67eff950aeff  a530_zap-pro.elf
e3445fe6aa3e14cb45b593e5d7a1fb786f22f0b5bc82862b4776b17fe2a086950d6f59c310359d77605d1d0cba6beaaf0879939c5239d7dc6248a4b03dc75a4a  20-adreno-gpu-firmware.files
8deca102436a21d97911f9a2a819ec52991a3089a7c08acc1c919791a6dc77e2ebb9902ada7be9370cb9160f0b8a83b3b402c034f6da97f0c3245a9577570d47  board-2.json
"
