From 01b579a527b5c77e6adfbb2c277fb2c7cc158b8b Mon Sep 17 00:00:00 2001
From: Paolo Sabatino <paolo.sabatino@gmail.com>
Date: Thu, 10 Feb 2022 21:30:54 +0000
Subject: [PATCH] add broadcom bcm43342 chip id

---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c       | 2 ++
 drivers/net/wireless/broadcom/brcm80211/include/brcm_hw_ids.h | 1 +
 2 files changed, 3 insertions(+)

diff --git a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
index 8effeb7a726..f45c1056e42 100644
--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
@@ -609,6 +609,7 @@ BRCMF_FW_DEF(4329, "brcmfmac4329-sdio");
 BRCMF_FW_DEF(4330, "brcmfmac4330-sdio");
 BRCMF_FW_DEF(4334, "brcmfmac4334-sdio");
 BRCMF_FW_DEF(43340, "brcmfmac43340-sdio");
+BRCMF_FW_DEF(43342, "brcmfmac43342-sdio");
 BRCMF_FW_DEF(4335, "brcmfmac4335-sdio");
 BRCMF_FW_DEF(43362, "brcmfmac43362-sdio");
 BRCMF_FW_DEF(4339, "brcmfmac4339-sdio");
@@ -642,6 +643,7 @@ static const struct brcmf_firmware_mapping brcmf_sdio_fwnames[] = {
 	BRCMF_FW_ENTRY(BRCM_CC_4334_CHIP_ID, 0xFFFFFFFF, 4334),
 	BRCMF_FW_ENTRY(BRCM_CC_43340_CHIP_ID, 0xFFFFFFFF, 43340),
 	BRCMF_FW_ENTRY(BRCM_CC_43341_CHIP_ID, 0xFFFFFFFF, 43340),
+	BRCMF_FW_ENTRY(BRCM_CC_43342_CHIP_ID, 0xFFFFFFFF, 43342),
 	BRCMF_FW_ENTRY(BRCM_CC_4335_CHIP_ID, 0xFFFFFFFF, 4335),
 	BRCMF_FW_ENTRY(BRCM_CC_43362_CHIP_ID, 0xFFFFFFFE, 43362),
 	BRCMF_FW_ENTRY(BRCM_CC_4339_CHIP_ID, 0xFFFFFFFF, 4339),
diff --git a/drivers/net/wireless/broadcom/brcm80211/include/brcm_hw_ids.h b/drivers/net/wireless/broadcom/brcm80211/include/brcm_hw_ids.h
index 9d81320164c..71de0dce4f4 100644
--- a/drivers/net/wireless/broadcom/brcm80211/include/brcm_hw_ids.h
+++ b/drivers/net/wireless/broadcom/brcm80211/include/brcm_hw_ids.h
@@ -27,6 +27,7 @@
 #define BRCM_CC_4334_CHIP_ID		0x4334
 #define BRCM_CC_43340_CHIP_ID		43340
 #define BRCM_CC_43341_CHIP_ID		43341
+#define BRCM_CC_43342_CHIP_ID		43342
 #define BRCM_CC_43362_CHIP_ID		43362
 #define BRCM_CC_4335_CHIP_ID		0x4335
 #define BRCM_CC_4339_CHIP_ID		0x4339
-- 
2.30.2

