# Archived: not needed by mainline kernel, describes only the hardware
maintainer=""
pkgname=firmware-kobo-clara-downstream
pkgver=4.26.16704
pkgrel=0
pkgdesc="Kobo Clara firmware"
url="https://wiki.mobileread.com/wiki/Kobo_Firmware_Releases"
arch="armv7"
license="proprietary"
options="!check !archcheck !tracedeps pmb:cross-native"

source="
	https://download.kobobooks.com/firmwares/kobo7/Feb2021/kobo-update-4.26.16704.zip
	hwcfg.bin
"

# Print given number as bytes in 32-bit little-endian
_le32() {
	printf "%08x" "$1" | sed -E 's/(..)(..)(..)(..)/\\x\4\\x\3\\x\2\\x\1/'
}
# Print the magic header for the given file for Kobo u-boot
_print_header() {
	length=$(stat -L -c %s "$1")
	dd bs=496 count=1 if=/dev/zero
	printf '\xff\xf5\xaf\xff\x78\x56\x34\x12%b\x00\x00\x00\x00' "$(_le32 "$length")"
}

build() {
	# Prepend a header to each firmware file loaded by u-boot
	for fw in hwcfg upgrade/mx6sll-ntx/ntxfw-E60K00 ; do
		out="$srcdir/$fw+header.bin"
		_print_header "$srcdir/$fw.bin" > "$out"
		cat "$srcdir/$fw.bin" >> "$out"
	done
}

package() {
	# Hardware description struct, passed to kernel by u-boot
	# See https://misc.andi.de1.cc/kobo/
	install -Dm644 "$srcdir/hwcfg+header.bin" \
		"$pkgdir/usr/share/firmware/kobo-clara/hwcfg+header.bin"

	# Value table for the 2-color lm3630 frontlight, passed to kernel by u-boot
	install -Dm644 "$srcdir/upgrade/mx6sll-ntx/ntxfw-E60K00+header.bin" \
		"$pkgdir/usr/share/firmware/kobo-clara/ntxfw-E60K00+header.bin"
}

sha512sums="
c1f89e630777ebad282ad77f40355b5fb50ad3c8fa57ed624b89d53d4fbb788783ed60f85f6f848f786c8c5ea7dcb913d16446fa2a87d68f033277272799d149  kobo-update-4.26.16704.zip
f7820b6c4624bab4bea92a0e2732cdaae8a37fbbe2ef823e61c48bb3e2400c70f7ee3c7945e7826f01653ba65f9a4034e884b985518fbcb84c8759c9c6351fad  hwcfg.bin
"
