# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Xiaomi Redmi Note 8 Pro"
deviceinfo_manufacturer="Xiaomi"
deviceinfo_codename="xiaomi-begonia"
deviceinfo_year="2019"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_chassis="handset"
deviceinfo_drm="true"
deviceinfo_external_storage="true"

# Bootimg related
deviceinfo_bootimg_custom_args="--header_version 2 --dtb /boot/dtbs/mediatek/mt6785-xiaomi-begonia.dtb --recovery_dtbo /boot/empty.dtbo"
deviceinfo_generate_bootimg="true"

# Flashing related
deviceinfo_flash_kernel_on_update="true"
deviceinfo_flash_method="fastboot"
deviceinfo_flash_offset_base="0x40078000"
deviceinfo_flash_offset_dtb="0x0bc08000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x07c08000"
deviceinfo_flash_offset_second="0xbff88000"
deviceinfo_flash_offset_tags="0x0bc08000"
deviceinfo_flash_pagesize="2048"
deviceinfo_flash_sparse="true"

# Required for devices using UFS as storage (instead of e.g. eMMC)
deviceinfo_rootfs_image_sector_size="4096"
