From 1506286d8c16d785be82821ec85f43dffa389b83 Mon Sep 17 00:00:00 2001
From: Oliver Smith <ollieparanoid@postmarketos.org>
Date: Tue, 20 Oct 2020 11:11:48 +0200
Subject: [PATCH] dts: pinetab: add missing ohci1

ohci1 is the low-speed variant of the usb port.
Original patch by Icenowy Zheng.

Cherry picked from here, but this isn't the original patch either:
https://gitlab.com/pine64-org/linux/-/commit/69ae7087ec51b09bb6a0afb53dddb5eb030b3236
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
index 419fe19b4a6f..e30034a1553b 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
@@ -311,6 +311,10 @@ &ohci0 {
 	status = "okay";
 };
 
+&ohci1 {
+	status = "okay";
+};
+
 &pwm {
 	status = "okay";
 };
-- 
2.52.0

