maintainer="m0rf30 <morf3089@gmail.com>"
pkgname=firmware-xiaomi-tulip
pkgver=4
pkgrel=0
_commit="c8f750d4cdd8c5353c4aaa423f81774c63f87d27"
pkgdesc="Firmware files for Xiaomi Redmi Note 6 Pro"
url="https://postmarketos.org"
arch="aarch64"
license="proprietary"
options="!strip !check !archcheck !spdx !tracedeps pmb:cross-native"
makedepends="qca-swiss-army-knife"
source="$pkgname-$_commit.tar.gz::https://github.com/M0Rf30/postmarketos-vendor-xiaomi-tulip/archive/$_commit.tar.gz"

builddir="$srcdir/postmarketos-vendor-xiaomi-tulip-$_commit"
_fwdir="/lib/firmware"

package() {
	ath10k-fwencoder --create \
		--features=wowlan,no-nwifi-decap-4addr-padding,allows-mesh-bcast,mgmt-tx-by-ref,non-bmi,single-chan-info-per-channel  \
		--set-wmi-op-version=tlv --set-htt-op-version=tlv \
		--set-fw-api=5
	install -Dm644 firmware-5.bin -t "$pkgdir/$_fwdir/ath10k/WCN3990/hw1.0/"
	install -Dm644 ath10k/WCN3990/hw1.0/board-2.bin -t "$pkgdir/$_fwdir/ath10k/WCN3990/hw1.0/"
	install -Dm644 qcom/a512_zap.elf "$pkgdir/$_fwdir/postmarketos/a512_zap.mbn"
}

sha512sums="
fd36819cabb028973015587e4193642e7c36b2321181a1c3dc7631fcfe51e7e736f4679665d4e4ad2eef8ddd4fe541a8a15e93189822702e23463a43023fe549  firmware-xiaomi-tulip-c8f750d4cdd8c5353c4aaa423f81774c63f87d27.tar.gz
"
