From 6060a61a28db987c10f8bc1ff9781455ea4ba220 Mon Sep 17 00:00:00 2001
From: Snejp <bartosz.dudziak@snejp.pl>
Date: Thu, 4 Jun 2020 15:07:31 +0200
Subject: [PATCH 5/5] alternative patch to fix refresh rate

---
 drivers/video/msm/mdss/mdss_fb.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/video/msm/mdss/mdss_fb.c b/drivers/video/msm/mdss/mdss_fb.c
index 2898eede..26855ce7 100644
--- a/drivers/video/msm/mdss/mdss_fb.c
+++ b/drivers/video/msm/mdss/mdss_fb.c
@@ -1433,7 +1433,7 @@ static int mdss_fb_register(struct msm_fb_data_type *mfd)
 	var->left_margin = panel_info->lcdc.h_back_porch;
 	var->right_margin = panel_info->lcdc.h_front_porch;
 	var->hsync_len = panel_info->lcdc.h_pulse_width;
-	var->pixclock = panel_info->clk_rate / 1000;
+	var->pixclock = 1000000 / 60;
 
 	/* id field for fb app  */
 
-- 
2.25.1

