# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Samsung Galaxy S21 FE 5G"
deviceinfo_manufacturer="Samsung"
deviceinfo_codename="samsung-r9q2"
deviceinfo_year="2022"
deviceinfo_dtb="qcom/sm8350-samsung-r9q2"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_chassis="handset"
deviceinfo_external_storage="false"

# Bootloader related
deviceinfo_flash_method="heimdall-bootimg"
#deviceinfo_kernel_cmdline="console=null androidboot.hardware=qcom androidboot.memcg=1 lpm_levels.sleep_disabled=1 video=vfb:640x400,bpp=32,memsize=3072000 msm_rtb.filter=0x237 service_locator.enable=1 androidboot.usbcontroller=a600000.dwc3 swiotlb=2048 loop.max_part=7 cgroup.memory=nokmem,nosocket firmware_class.path=/vendor/firmware_mnt/image printk.devkmsg=on pcie_ports=compat cpuinfo.chipname=SM8350 panic=4"
deviceinfo_kernel_cmdline="video=vfb:640x400,bpp=32,memsize=3072000 console=tty0 PMOS_NOSPLASH loop.max_part=7"
deviceinfo_generate_bootimg="true"
deviceinfo_flash_pagesize="4096"
deviceinfo_bootimg_qcdt="false"
deviceinfo_header_version="3"
deviceinfo_flash_heimdall_partition_kernel="BOOT"
deviceinfo_flash_heimdall_partition_rootfs="USERDATA"
deviceinfo_flash_sparse="true"
deviceinfo_create_initfs_extra="true"

deviceinfo_rootfs_image_sector_size="4096"
deviceinfo_append_dtb="true"
